**Ricoh Streamline NX (SLNX)**

**SLNX license (Per MFP)**

|  |  |  |
| --- | --- | --- |
| No. | Product Code | Description |
| 1 | 421091 | SLNX Base License |
| 2 | 421106 | SLNX Secure Print License  |
| 3 | 421121 | SLNX Scan & Capture License |
| 4 | 421190/421185 | SLNX Maintenance & Support License |
| 5 | RDR-805H1BKU-AP-5Y | RFIDeas USB Card Reader |
| 6 | LOCAL MAINTENANCE | Ricoh Software Maintenance & Support |
| 7 | LOCAL PROFESSIONAL SERVICES | Ricoh Software Professional Services |

***\*Please include card reader cover to hide the card reader underneath***

***\*SLNX server has been setup and managed by TE Connectivity Singapore***

**Scope:**

* **Ricoh Local OpCo to assign an engineer trained in Streamline NX**
* TE Connectivity will provide SLNX admin access to local Ricoh OpCo
* Local Ricoh OpCo to configure network connectivity on MFP, enable CUMIN. Install card reader cover.
* Local Ricoh OpCo to install card reader to MFP. Please upload the configuration file to the card reader using RF Ideas Configuration Utility Tool



* There are SLNX embedded profiles created in SLNX.
* Local Ricoh OpCo will duplicate the profile for the local country usage.
* Local Ricoh OpCo to install SLNX embedded and enable remote panel operation on MFP
* Local Ricoh OpCo to conduct testing with TE
	+ Test card authentication/registration
	+ Test print release
	+ Test scan-to-me

***\*Synchronization with Active Directory has already been configured.***

***\*Print queue has been created. One print queue for the APAC region***

***\*For any technical queries, please reach out to Joseph Seah (******josephseah@ricoh.sg******) and Patrick Ho (patrickho@ricoh.sg)***